IFC building model
Schema: "IFC4"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2018-02-28T14:20:01"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20170117_1200(x64) - Exporter 16.0.1205.0 - Default UI"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "michele.mollet@cadcompany.nl" of Organization (no name given)
  Owner history of Person "michele.mollet@cadcompany.nl" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 1519823995 (2018-02-28T13:19:55Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  PRESSUREUNIT: PASCAL

Spatial structure
IFCPROJECT | long name "C:\Users\mmt\Documents\01_Bestanden\01_Structure\Klanten\xxxxxxx - A.O. Smith 2018\In progress\Indirect-Water-Heater_AO_Smith-ITS-400_B_B.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 3 elements
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Indirect-Water-Heater_AO_Smith-ITS-400_B_B" | object type "Indirect-Water-Heater_AO_Smith-ITS-400_B_B" | names: "Indirect-Water-Heater_AO_Smith-ITS-400_B_B:Indirect-Water-Heater_AO_Smith-ITS-400_B_B:10224" | material: materials ("RAL 9005", "Ral 9006 - Insulation", "Ral 9016") | property sets: Pset_BuildingElementProxyCommon, Pset_ManufacturerTypeInformation, Constraints, Dimensions, Identity Data, Mechanical
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "R1" | object type "R1" | names: "Warm water:R1:10225" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Identity Data, Other, Phasing
          1 x IFCBUILDINGELEMENTPROXY | type IFCBUILDINGELEMENTPROXYTYPE "Workspace" | object type "Workspace" | names: "Workspace:Workspace:10226" | material: "Workspace" | property sets: Pset_BuildingElementProxyCommon, Constraints, Dimensions, Other, Phasing

Types
  IFCBUILDINGELEMENTPROXYTYPE "Indirect-Water-Heater_AO_Smith-ITS-400_B_B" | 1 occurrence | material: materials ("RAL 9005", "Ral 9006 - Insulation", "Ral 9016") | property sets: Dimensions, General, Identity Data, Mechanical - Flow, Model Properties, Other
  IFCBUILDINGELEMENTPROXYTYPE "R1" | 1 occurrence | property sets: Identity Data, Other
  IFCBUILDINGELEMENTPROXYTYPE "Workspace" | 1 occurrence | material: "Workspace" | property sets: Identity Data, Other

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Indirect-Water-Heater_AO_Smith-ITS-400_B_B: Indirect-Water-Heater_AO_Smith-ITS-400_B_B" (IFCLABEL)
    Family and Type = "Indirect-Water-Heater_AO_Smith-ITS-400_B_B: Indirect-Water-Heater_AO_Smith-ITS-400_B_B" (IFCLABEL)
    Type = "Indirect-Water-Heater_AO_Smith-ITS-400_B_B: Indirect-Water-Heater_AO_Smith-ITS-400_B_B" (IFCLABEL)
    Type Id = "Indirect-Water-Heater_AO_Smith-ITS-400_B_B: Indirect-Water-Heater_AO_Smith-ITS-400_B_B" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Mechanical Equipment" (IFCLABEL)
    Family = "Warm water: R1" (IFCLABEL)
    Family and Type = "Warm water: R1" (IFCLABEL)
    Type = "Warm water: R1" (IFCLABEL)
    Type Id = "Warm water: R1" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Category = "Generic Models" (IFCLABEL)
    Family = "Workspace: Workspace" (IFCLABEL)
    Family and Type = "Workspace: Workspace" (IFCLABEL)
    Type = "Workspace: Workspace" (IFCLABEL)
    Type Id = "Workspace: Workspace" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Indirect-Water-Heater_AO_Smith-ITS-400_B_B" (IFCTEXT)
    Pressure Loss - top heat exchanger 80ºC/60ºC = 3000. (IFCPRESSUREMEASURE) [PASCAL]
  Other | properties | on 1 type object
    Category = "Mechanical Equipment" (IFCLABEL)
    Family Name = "Warm water" (IFCTEXT)
  Other: 1 more content on 0 objects not shown
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Indirect-Water-Heater_AO_Smith-ITS-400_B_B" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "R1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    IsExternal = FALSE (IFCBOOLEAN)
    Reference = "Workspace" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1655. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "None" (IFCTEXT)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 6.408632019854 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.736954409637151 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 0.0240655263725559 (IFCAREAMEASURE) [SQUARE_METRE]
    Diameter = 740. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.000810693486417095 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Area = 23.1787062804012 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 23.7805092601345 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Workspace Diameter = 1740. (IFCLENGTHMEASURE) [MILLI METRE]
    workspace_height = 2500. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    Diameter (with insulation) = 740. (IFCLENGTHMEASURE) [MILLI METRE]
    Diameter (without insulation) = 600. (IFCLENGTHMEASURE) [MILLI METRE]
    Height (with insulation) = 1710. (IFCLENGTHMEASURE) [MILLI METRE]
    Height (without insulation) = 1655. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Cold Water Inlet = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    Height Warm Water Outlet = 1655. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Diameter = 1740. (IFCLENGTHMEASURE) [MILLI METRE]
    Workspace Height = 2710. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "D3010" (IFCTEXT)
    Assembly Description = "Energy Supply" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    BIM Content Developer URL = "http://www.cadcompany.be/" (IFCTEXT)
    CE-PIN = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "Indirecte Boiler met 2 warmtewisselaars" (IFCTEXT)
    Destination / Counrty = "België" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Manufacturer Number = "E 7110 E 7110 E 7110" (IFCTEXT)
    Model = "ITS 400 B B" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Product Documentation Link = "https://www.aosmithinternational.com/wp-content/uploads/Specsheet_ITS_BENL.pdf" (IFCTEXT)
    Product Instruction Link = "https://www.aosmithinternational.com/wp-content/uploads/Instructiehandleiding_ITS-400-1000_BENL.pdf" (IFCTEXT)
    Serial Number = "8717449181536" (IFCTEXT)
    Type Name = "Indirect-Water-Heater_AO_Smith-ITS-400_B_B" (IFCTEXT)
    URL = "www.aosmith.be" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "R1" (IFCTEXT)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Name = "Workspace" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    System Classification = "Hydronic Supply" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Phasing | properties | on 3 objects (3 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
    Reference = "Project Information" (IFCIDENTIFIER)
  General | properties | on 1 type object
    1e Maintenance (check-up) = "3 maanden na installatie" (IFCTEXT)
    2nd Maintenance (general maintenance) = "12 maanden na installatie" (IFCTEXT)
    Maintenance Interval = "12 maanden" (IFCTEXT)
    Packaging Height = 1850. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Length = 780. (IFCLENGTHMEASURE) [MILLI METRE]
    Packaging Width = 780. (IFCLENGTHMEASURE) [MILLI METRE]
    Transport Weight = 156. (IFCREAL)
    Type of Packaging = "Plastic en Hout" (IFCTEXT)
    Warranty on Parts = "12 maanden" (IFCTEXT)
    Warranty on Tank = "36 maanden" (IFCTEXT)
  Mechanical - Flow | properties | on 1 type object
    Draw-off Capacity @ ΔT = 28°C after 120 min. = 6.095 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 28°C after 30 min. = 1.994 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 28°C after 60 min. = 3.361 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 28°C after 90 min. = 4.728 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 120 min. = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 30 min. = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 60 min. = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 44°C after 90 min. = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 120 min. = 3.413 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 30 min. = 1.117 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 60 min. = 1.882 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 50°C after 90 min. = 2.648 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 120 min. = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 30 min. = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 60 min. = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 55°C after 90 min. = 0. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 120 min. = 2.438 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 30 min. = 0.798 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 60 min. = 1.344 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Draw-off Capacity @ ΔT = 70°C after 90 min. = 1.891 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Heating Up Time @ ΔT = 28°C = "8" (IFCTEXT)
    Heating Up Time @ ΔT = 44°C = "" (IFCTEXT)
    Heating Up Time @ ΔT = 50°C = "15" (IFCTEXT)
    Heating Up Time @ ΔT = 55°C = "" (IFCTEXT)
    Heating Up Time @ ΔT = 70°C = 21 (IFCINTEGER)
    Recovery Rate @ ΔT = 28°C (ltr/hr) = 2734. (IFCREAL)
    Recovery Rate @ ΔT = 44°C (ltr/hr) = 0. (IFCREAL)
    Recovery Rate @ ΔT = 50°C (ltr/hr) = 1531. (IFCREAL)
    Recovery Rate @ ΔT = 55°C (ltr/hr) = 0. (IFCREAL)
    Recovery Rate @ ΔT = 70°C (ltr/hr) = 1093. (IFCREAL)
  Model Properties | properties | on 1 type object
    Empty Weight = 145. (IFCREAL)
    Flow Rate - bottom heat exchanger 80ºC/60ºC = 2236. (IFCREAL)
    Flow Rate - top heat exchanger 80ºC/60ºC = 1591. (IFCREAL)
    Insulation Thickness = 70. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. Operating Pressure - bottom heat exchanger = 1600000. (IFCPRESSUREMEASURE) [PASCAL]
    Max. Operating Pressure - tank = 1000000. (IFCPRESSUREMEASURE) [PASCAL]
    Max. Operating Pressure - top heat exchanger = 1600000. (IFCPRESSUREMEASURE) [PASCAL]
    Max. Tempature - bottom heat exchanger = 110. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Max. Tempature - top heat exchanger = 110. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Max. Temperature - tank = 95. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Noise-level = "" (IFCTEXT)
    Nominal Output - bottom heat exchanger = 52000. (IFCPOWERMEASURE) [WATT]
    Nominal Output - top heat exchanger = 37000. (IFCPOWERMEASURE) [WATT]
    Operating Weight = 527. (IFCREAL)
    Pressure Loss - bottom heat exchanger 80ºC/60ºC = 7800. (IFCPRESSUREMEASURE) [PASCAL]
    Stand-by Loss - daily (Watt/24H) = 0. (IFCREAL)
    Stand-by Loss = 0. (IFCPOWERMEASURE) [WATT]
    Storage Capacity - bottom heat exchanger = 9.9 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Storage Capacity - tank = 382. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Storage Capacity - top heat exchanger = 6.9 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Surface bottom heat Exchanger = 1.64 (IFCAREAMEASURE) [SQUARE_METRE]
    Surface top heat Exchanger = 1.15 (IFCAREAMEASURE) [SQUARE_METRE]
  Plumbing | properties | on 1 type object
    Cold Water Connection R = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    Hot / Warm Water Connection R = 50.8 (IFCLENGTHMEASURE) [MILLI METRE]
    T&P Connection Rp = 19.05 (IFCLENGTHMEASURE) [MILLI METRE]