IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2015-04-20T15:49:09"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "BTN" of Organization (no name given)
  Owner history of Person "BTN" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 13 elements
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-35-130_PF" | object type "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-35-130_PF" | names: "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-35-130_PF:Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-35-130_PF:187612" | material: "Workspace 3D" | property sets: Phasing, Constraints, Other, Mechanical, Identity Data, Pset_ManufacturerTypeInformation
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "10.Boiler TWI" | object type "10.Boiler TWI" | names: "01. Boiler TWI:10.Boiler TWI:187614" | material: materials ("RAL 9005", "RAL 9006") | property sets: Phasing, Constraints, Identity Data
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "01.Chimney Pipe" | object type "01.Chimney Pipe" | names: "02. Chimney Pipe:01.Chimney Pipe:187616" | material: materials ("Aluminium") | property sets: Identity Data, Constraints, Phasing
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "09.Control panel TWI" | object type "09.Control panel TWI" | names: "09.Control panel TWI:09.Control panel TWI:187617" | material: materials ("RAL 9005", "Aluminium", "Green light", "Yellow light", "Red light", "Twister - Control panel") | property sets: Phasing, Constraints, Identity Data
          2 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "08.Cover plate 2" | object type "08.Cover plate 2" | names: "05. Cover plate:08.Cover plate 2:187618", "05. Cover plate:08.Cover plate 2:187619" | material: "RAL 9005" | property sets: Constraints, Identity Data, Phasing
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "08. Product sticker - Twister TWI" | object type "08. Product sticker - Twister TWI" | names: "08. Product sticker - Twister TWI:08. Product sticker - Twister TWI:187620" | material: "RAL 9011" | property sets: Identity Data, Constraints, Phasing
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "03.Gas control (external)" | object type "03.Gas control (external)" | names: "05.Gas control (external):03.Gas control (external):187621" | material: materials ("Aluminium", "RAL 9005") | property sets: Identity Data, Constraints, Phasing
          2 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "05. T&P valve (internal)" | object type "05. T&P valve (internal)" | names: "07. T&P valve (internal):05. T&P valve (internal):187622", "07. T&P valve (internal):05. T&P valve (internal):187626" | material: "RAL 9011" | property sets: Identity Data, Constraints, Phasing, Pset_ManufacturerTypeInformation
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "01. Water control (external)" | object type "01. Water control (external)" | names: "04. Water control (external):01. Water control (external):187623" | material: materials ("Rubber", "Aluminium") | property sets: Identity Data, Constraints, Phasing
          2 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "01. Water control (external)" | object type "01. Water control (external)" | names: "04. Water control (external):01. Water control (external):187624", "04. Water control (external):01. Water control (external):187625" | material: materials ("Rubber", "Aluminium") | property sets: Identity Data, Constraints, Phasing

Types
  IFCBOILERTYPE "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-35-130_PF" | element type "Condensing-Storage-Water-Heater-Gas-AO_Smith-TWI-35-130_PF" | 1 occurrence | material: "Workspace 3D"
  IFCBOILERTYPE "10.Boiler TWI" | element type "10.Boiler TWI" | 1 occurrence | material: materials ("RAL 9005", "RAL 9006")
  IFCBOILERTYPE "01.Chimney Pipe" | element type "01.Chimney Pipe" | 1 occurrence | material: materials ("Aluminium")
  IFCBOILERTYPE "09.Control panel TWI" | element type "09.Control panel TWI" | 1 occurrence | material: materials ("RAL 9005", "Aluminium", "Green light", "Yellow light", "Red light", "Twister - Control panel")
  IFCBOILERTYPE "08.Cover plate 2" | element type "08.Cover plate 2" | 2 occurrences | material: "RAL 9005"
  IFCBOILERTYPE "08. Product sticker - Twister TWI" | element type "08. Product sticker - Twister TWI" | 1 occurrence | material: "RAL 9011"
  IFCBOILERTYPE "03.Gas control (external)" | element type "03.Gas control (external)" | 1 occurrence | material: materials ("Aluminium", "RAL 9005")
  IFCBOILERTYPE "05. T&P valve (internal)" | element type "05. T&P valve (internal)" | 2 occurrences | material: "RAL 9011"
  IFCBOILERTYPE "01. Water control (external)" | element type "01. Water control (external)" | 1 occurrence | material: materials ("Rubber", "Aluminium")
  IFCBOILERTYPE "01. Water control (external)" | element type "01. Water control (external)" | 2 occurrences | material: materials ("Rubber", "Aluminium")

Property sets
  Constraints | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 30. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 100. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1075. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1040. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1.11311663148492 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints: 3 more contents on 3 objects not shown
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Phasing | properties | on 13 objects (13 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Workspace = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    System Classification = "Domestic Hot Water,Hydronic Supply,Other,Hydronic Supply,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Pression Différentielle d'Ouverture de l'Interrupteur de Pression = 213.36 (IFCREAL)
  Identity Data | properties | on 10 objects (10 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
  Identity Data | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Manufacturer = "A.O. Smith" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Comments = "T&P valve (internal)" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "5" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "6" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "7" (IFCTEXT)
  Identity Data: 10 more contents on 10 objects not shown
  Pset_ManufacturerTypeInformation | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "A.O. Smith" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Green Building Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    NOX-émissions (ven air, 0% O2) = "" (IFCTEXT)
    NOX-émissions = "" (IFCTEXT)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Diamètre = 730. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre Cheminée - Boiler = "100/150 mm/mm" (IFCTEXT)
    Diamètre Cheminée - Système Concentrique = "100/150 mm/mm" (IFCTEXT)
    Diamètre Cheminée - Système Parallèle = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur = 1270. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Conduit d'Alimentation en Air = 385. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Conduit d'Évacuation des Fumées = 385. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de l'Alimentation en eau Froide = 400. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de la Sortie d'eau Chaude = 1270. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur du Raccordement au Gaz = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Mechanical - Flow | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Débit de vidage en Continu à ΔT = 28°C = 1.2 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 44°C = 0.71 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 50°C = 0.62 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 55°C = 0.57 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 70°C = 0.45 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage à ΔT = 28°C après 120 min. = 84.7552001315726 (IFCREAL)
    Débit de vidage à ΔT = 28°C après 30 min. = 25.7797067066867 (IFCREAL)
    Débit de vidage à ΔT = 28°C après 60 min. = 45.9090667379352 (IFCREAL)
    Débit de vidage à ΔT = 28°C après 90 min. = 67.0978667708283 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 120 min. = 52.9720000822329 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 30 min. = 15.8916000246699 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 60 min. = 28.2517333771909 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 90 min. = 42.3776000657863 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 120 min. = 49.440533410084 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 30 min. = 13.4195733541657 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 60 min. = 24.3671200378271 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 90 min. = 35.3146667214886 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 120 min. = 42.3776000657863 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 30 min. = 12.0069866853061 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 60 min. = 21.8950933673229 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 90 min. = 31.7832000493397 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 120 min. = 32.1363467165546 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 30 min. = 8.82866668037215 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 60 min. = 16.5978933590996 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 90 min. = 24.3671200378271 (IFCREAL)
    Temps de réchauffement à ΔT = 28°C = "7" (IFCTEXT)
    Temps de réchauffement à ΔT = 44°C = "11" (IFCTEXT)
    Temps de réchauffement à ΔT = 50°C = "12" (IFCTEXT)
    Temps de réchauffement à ΔT = 55°C = "14" (IFCTEXT)
    Temps de réchauffement à ΔT = 70°C = "17" (IFCTEXT)
  Electrical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    (Contrôle supplémentaires) Fréquence secteur (± 1 Hz) = 0. (IFCREAL)
    (Contrôle supplémentaires) Phase = 1 (IFCINTEGER)
    (Contrôle supplémentaires) Puissance Électrique Absorbée = 0. (IFCREAL)
    (Contrôle supplémentaires) Tension d'Alimentation (-15%, +10%) = 0. (IFCREAL)
    Fréquence secteur (± 1 Hz) = 50. (IFCREAL)
    Phase = 1 (IFCINTEGER)
    Puissance Électrique Absorbée = 2152.78208334194 (IFCREAL)
    Tension d'Alimentation (-15%, +10%) = 2475.69939584324 (IFCREAL)
  Model Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    CO2-émissions (tol. ± 1.0) = "11.9/10.0" (IFCTEXT)
    Capacité = 4.55559200707203 (IFCREAL)
    Charge Maximale au Sol = 199. (IFCREAL)
    Charge Nominale (Valeur Inférieure) = "39000.0/34000.0" (IFCTEXT)
    Charge Nominale (Valeur Supérieure) = "42300.0/37000.0" (IFCTEXT)
    Consommation de Gaz - Masse = "3.10/2.60" (IFCTEXT)
    Consommation de Gaz - Volume = 0. (IFCREAL)
    Epaisseur d'Isolation = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Niveau du Son = "51" (IFCTEXT)
    Pertes en Veille - tous les jours (24h) = 0. (IFCREAL)
    Pertes en Veille = 0. (IFCREAL)
    Poids à vide = 70. (IFCREAL)
    Pression Amont de Gaz = "3000/3700" (IFCTEXT)
    Pression de Fonctionnement Maximale = 243840. (IFCREAL)
    Production Nominale = "41300.0/36000.0" (IFCTEXT)
    Température Maximale des Fumées = 338.15 (IFCREAL)
    Valeur Défaut du Thermostat de Régulation = 338.15 (IFCREAL)
    Valeur Manimale du Thermostat de Régulation = 283.15 (IFCREAL)
    Valeur Maximale du Thermostat de Régulation = 358.15 (IFCREAL)
  Plumbing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Raccord Robinet de Vidange = 0.0625 (IFCREAL)
    Raccord d'Alimentation en Eau Froide = 0.0833333333333333 (IFCREAL)
    Raccord de Gaz = 0.0416666666666667 (IFCREAL)
    Raccord de Sortie d'Eau Chaude = 0.0833333333333333 (IFCREAL)
    Raccord de la Soupape de Vidange = 0.0833333333333333 (IFCREAL)
    Raccord Évacuation de la Condensation = 1. (IFCLENGTHMEASURE) [MILLI METRE]
  Energy Analysis | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Rendement (Hi, acc. NEN-EN 89 - 1999) = 106. (IFCREAL)
    Rendement (Hs, acc. NEN-EN 89 - 1999) = 95. (IFCREAL)
    Rendement Saisonnier (Hs) = 91. (IFCREAL)
  General | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    1er Entretien (check-up) = "3 mois après l'installation" (IFCTEXT)
    2ème Entretien (Entretien Général) = "12 mois après l'installation" (IFCTEXT)
    Garantie Pièces = "12 mois" (IFCTEXT)
    Garantie sur la Cuve = "36 mois" (IFCTEXT)
    Hauteur d'Emballage = 1400. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur d'Emballage = 780. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids de Transport = 88. (IFCREAL)
    Profondeur d'Emballage = 870. (IFCLENGTHMEASURE) [MILLI METRE]
    Type d'Emballage = "Plastique Emballage Rétractable, Carton et Bois" (IFCTEXT)
    l'Intervalle d'Entretien = "12 mois" (IFCTEXT)