IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2015-05-11T12:40:51"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "BTN" of Organization (no name given)
  Owner history of Person "BTN" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 8 elements
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_50_F" | object type "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_50_F" | names: "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_50_F:Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_50_F:415678" | material: materials ("XX_AO Smith - RAL 1036", "RAL 9011", "XX_AO Smith - RAL 9011", "Workspace 3D") | property sets: Phasing, Electrical - Loads, Constraints, Identity Data, Other, Mechanical
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "09.Boiler - 705mm" | object type "09.Boiler - 705mm" | names: "09.Boiler - 705mm:09.Boiler - 705mm:415680" | material: "RAL 9006" | property sets: Identity Data, Constraints, Phasing, Pset_ManufacturerTypeInformation, Dimensions
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "02_Water control (external)" | object type "02_Water control (external)" | names: "02_Water control (external):02_Water control (external):415681" | material: materials ("Rubber", "RAL 1036") | property sets: Constraints, Identity Data, Phasing, Pset_ManufacturerTypeInformation
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "04_Tank drain valve (external)" | object type "04_Tank drain valve (external)" | names: "04_Tank drain valve (external):04_Tank drain valve (external):415683" | material: materials ("XX_AO Smith - RAL 1036", "XX_AO Smith - Aluminium", "XX_AO Smith - RAL 3000") | property sets: Phasing, Identity Data, Constraints
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "06_Cleaning and inspection opening" | object type "06_Cleaning and inspection opening" | names: "06_Cleaning and inspection opening:06_Cleaning and inspection opening:415685" | material: "RAL 9011" | property sets: Identity Data, Constraints, Phasing, Pset_ManufacturerTypeInformation
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "10_Temperature sensor" | object type "10_Temperature sensor" | names: "10_Temperature sensor:10_Temperature sensor:415686" | material: "RAL 9011" | property sets: Identity Data, Phasing, Constraints
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "Condensation drainage (internal)" | object type "Condensation drainage (internal)" | names: "07_Condensation drainage (internal):Condensation drainage (internal):415687" | material: "XX_AO Smith - RAL 9005" | property sets: Identity Data, Phasing, Constraints
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "09_BCF 30-50-60 - Chimney Pipe" | object type "09_BCF 30-50-60 - Chimney Pipe" | names: "09_BCF 30-50-60 - Chimney Pipe:09_BCF 30-50-60 - Chimney Pipe:415688" | material: "Aluminium" | property sets: Identity Data, Phasing, Constraints

Types
  IFCBOILERTYPE "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_50_F" | element type "Condensing-Storage-Water-Heater-Gas_AO_Smith-BFC_50_F" | 1 occurrence | material: materials ("XX_AO Smith - RAL 1036", "RAL 9011", "XX_AO Smith - RAL 9011", "Workspace 3D")
  IFCBOILERTYPE "09.Boiler - 705mm" | element type "09.Boiler - 705mm" | 1 occurrence | material: "RAL 9006"
  IFCBOILERTYPE "02_Water control (external)" | element type "02_Water control (external)" | 1 occurrence | material: materials ("Rubber", "RAL 1036")
  IFCBOILERTYPE "04_Tank drain valve (external)" | element type "04_Tank drain valve (external)" | 1 occurrence | material: materials ("XX_AO Smith - RAL 1036", "XX_AO Smith - Aluminium", "XX_AO Smith - RAL 3000")
  IFCBOILERTYPE "06_Cleaning and inspection opening" | element type "06_Cleaning and inspection opening" | 1 occurrence | material: "RAL 9011"
  IFCBOILERTYPE "10_Temperature sensor" | element type "10_Temperature sensor" | 1 occurrence | material: "RAL 9011"
  IFCBOILERTYPE "Condensation drainage (internal)" | element type "Condensation drainage (internal)" | 1 occurrence | material: "XX_AO Smith - RAL 9005"
  IFCBOILERTYPE "09_BCF 30-50-60 - Chimney Pipe" | element type "09_BCF 30-50-60 - Chimney Pipe" | 1 occurrence | material: "Aluminium"

Property sets
  Constraints | properties | on 2 objects (2 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 160. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = -9.2932599030856 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 175. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 21.6134665205261 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 119.245800724402 (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints: 1 more content on 1 objects not shown
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Phasing | properties | on 8 objects (8 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Electrical - Loads | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Circuit Number = "" (IFCTEXT)
    Panel = "" (IFCTEXT)
  Identity Data | properties | on 4 objects (4 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "3" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "5" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Manufacturer = "A.O. Smith" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
    Type Comments = "Cleaning and inspection opening" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "8" (IFCTEXT)
  Identity Data: 7 more contents on 7 objects not shown
  Other | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Workspace = TRUE (IFCBOOLEAN)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    System Classification = "Domestic Cold Water,Other,Domestic Hot Water,Other,Domestic Cold Water,Power" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Pression Différentielle d'Ouverture de l'Interrupteur de Pression = 35.052 (IFCREAL)
  Pset_ManufacturerTypeInformation | properties | on 3 objects (3 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "A.O. Smith" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    A = 1910. (IFCLENGTHMEASURE) [MILLI METRE]
    K = 1566. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Diamètre = 705. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre Cheminée - Boiler = "100/150 mm/mm" (IFCTEXT)
    Diamètre Cheminée - Système Concentrique = "100/150 mm/mm" (IFCTEXT)
    Diamètre Cheminée - Système Parallèle = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur = 1910. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Conduit d'Alimentation en Air = 1905. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur Conduit d'Évacuation des Fumées = 1905. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de l'Alimentation en eau Froide = 160. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de la Sortie d'eau Chaude = 1910. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur du Raccordement au Gaz = 1815. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Model Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    CO2-émissions (tol. ± 1.0) = "9.00/9.20" (IFCTEXT)
    Capacité = 12.9957973535078 (IFCREAL)
    Charge Maximale au Sol = 582. (IFCREAL)
    Charge Nominale (Valeur Inférieure) = 505903.789585357 (IFCREAL)
    Charge Nominale (Valeur Supérieure) = 561876.123752248 (IFCREAL)
    Consommation de Gaz - Masse = 0. (IFCREAL)
    Consommation de Gaz - Volume = "5.00/5.80" (IFCTEXT)
    Epaisseur d'Isolation = 50. (IFCLENGTHMEASURE) [MILLI METRE]
    Niveau du Son = "45" (IFCTEXT)
    Pertes en Veille - tous les jours (24h) = 0. (IFCREAL)
    Pertes en Veille = 0. (IFCREAL)
    Poids à vide = 214. (IFCREAL)
    Pression Amont de Gaz = "2000/2500" (IFCTEXT)
    Pression de Fonctionnement Maximale = 243840. (IFCREAL)
    Production Nominale = 541424.693960499 (IFCREAL)
    Température Maximale des Fumées = 333.15 (IFCREAL)
    Valeur Défaut du Thermostat de Régulation = 338.15 (IFCREAL)
    Valeur Manimale du Thermostat de Régulation = 313.15 (IFCREAL)
    Valeur Maximale du Thermostat de Régulation = 353.15 (IFCREAL)
  General | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    1er Entretien (check-up) = "3 mois après l'installation" (IFCTEXT)
    2ème Entretien (Entretien Général) = "12 mois après l'installation" (IFCTEXT)
    Garantie Pièces = "12 mois" (IFCTEXT)
    Garantie sur la Cuve = "36 mois" (IFCTEXT)
    Hauteur d'Emballage = 2080. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur d'Emballage = 790. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids de Transport = 235. (IFCREAL)
    Profondeur d'Emballage = 950. (IFCLENGTHMEASURE) [MILLI METRE]
    Type d'Emballage = "Plastique Emballage Rétractable, Carton et Bois" (IFCTEXT)
    l'Intervalle d'Entretien = "12 mois" (IFCTEXT)
  Mechanical - Flow | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Débit de vidage en Continu à ΔT = 28°C = 1.6 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 44°C = 0.99 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 50°C = 0.87 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 55°C = 0.79 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage en Continu à ΔT = 70°C = 0.62 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Débit de vidage à ΔT = 28°C après 120 min. = 127.132800197359 (IFCREAL)
    Débit de vidage à ΔT = 28°C après 30 min. = 45.9090667379352 (IFCREAL)
    Débit de vidage à ΔT = 28°C après 60 min. = 74.160800115126 (IFCREAL)
    Débit de vidage à ΔT = 28°C après 90 min. = 98.881066820168 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 120 min. = 81.2237334594237 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 30 min. = 25.7797067066867 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 60 min. = 45.9090667379352 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 90 min. = 63.5664000986795 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 120 min. = 70.6293334429772 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 30 min. = 21.8950933673229 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 60 min. = 38.8461333936374 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 90 min. = 52.9720000822329 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 120 min. = 63.5664000986795 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 30 min. = 19.0699200296038 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 60 min. = 33.1957867181993 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 90 min. = 49.440533410084 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 120 min. = 45.9090667379352 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 30 min. = 13.0664266869508 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 60 min. = 23.6608267033974 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 90 min. = 34.6083733870588 (IFCREAL)
    Temps de réchauffement à ΔT = 28°C = "14" (IFCTEXT)
    Temps de réchauffement à ΔT = 44°C = "22" (IFCTEXT)
    Temps de réchauffement à ΔT = 50°C = "26" (IFCTEXT)
    Temps de réchauffement à ΔT = 55°C = "28" (IFCTEXT)
    Temps de réchauffement à ΔT = 70°C = "36" (IFCTEXT)
  Electrical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    (Contrôle supplémentaires) Fréquence secteur (± 1 Hz) = 0. (IFCREAL)
    (Contrôle supplémentaires) Phase = 1 (IFCINTEGER)
    (Contrôle supplémentaires) Puissance Électrique Absorbée = 0. (IFCREAL)
    (Contrôle supplémentaires) Tension d'Alimentation (-15%, +10%) = 0. (IFCREAL)
    Fréquence secteur (± 1 Hz) = 50. (IFCREAL)
    Phase = 1 (IFCINTEGER)
    Puissance Électrique Absorbée = 807.293281253229 (IFCREAL)
    Tension d'Alimentation (-15%, +10%) = 2475.69939584324 (IFCREAL)
  Green Building Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    NOX-émissions (ven air, 0% O2) = "29.0/29.0" (IFCTEXT)
    NOX-émissions = "52.0/52.0" (IFCTEXT)
  Plumbing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Raccord Robinet de Vidange = 0.0833333333333333 (IFCREAL)
    Raccord d'Alimentation en Eau Froide = 0.125 (IFCREAL)
    Raccord de Gaz = 0.0625 (IFCREAL)
    Raccord de Sortie d'Eau Chaude = 0.125 (IFCREAL)
    Raccord de la Soupape de Vidange = 0.0833333333333333 (IFCREAL)
    Raccord Évacuation de la Condensation = 40. (IFCLENGTHMEASURE) [MILLI METRE]
  Energy Analysis | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Rendement (Hi, acc. NEN-EN 89 - 1999) = 107. (IFCREAL)
    Rendement (Hs, acc. NEN-EN 89 - 1999) = 96. (IFCREAL)
    Rendement Saisonnier (Hs) = 96. (IFCREAL)