IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "0001"
Time stamp: "2015-05-11T12:37:57"
Preprocessor: "The EXPRESS Data Manager Version 5.01.0100.02.64mod : 6 Jun 2012"
Originating system: "20130308_1515(x64) - Exporter 2014.0.2013.0308 - Default UI"
Application: "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)"

People and organizations
  Person "BTN" of Organization (no name given)
  Owner history of Person "BTN" of Organization (no name given) | application "Autodesk Revit 2014 (ENU)" version "2014" identifier "Revit" by Organization "Autodesk Revit 2014 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  THERMODYNAMICTEMPERATUREUNIT: KELVIN
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  POWERUNIT: WATT

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 3 elements
          1 x IFCENERGYCONVERSIONDEVICE | type IFCBOILERTYPE "Indirect-Water-Heater_AO_Smith-IT-300_F_B" | object type "Indirect-Water-Heater_AO_Smith-IT-300_F_B" | names: "Indirect-Water-Heater_AO_Smith-IT-300_F_B:Indirect-Water-Heater_AO_Smith-IT-300_F_B:351010" | material: materials ("RAL 9005", "Ral 9006 - Insulation", "Ral 9016") | property sets: Mechanical, Identity Data, Constraints, Phasing, Pset_ManufacturerTypeInformation, Model Properties
          1 x IFCBUILDINGELEMENTPROXY | object type "R1" | names: "Warm water:R1:351012" | property sets: Constraints, Dimensions, Phasing, Pset_BuildingElementProxyCommon, Identity Data
          1 x IFCBUILDINGELEMENTPROXY | object type "Workspace" | names: "Workspace:Workspace:351013" | material: "Workspace" | property sets: Dimensions, Identity Data, Phasing, Constraints, Pset_BuildingElementProxyCommon

Types
  IFCBOILERTYPE "Indirect-Water-Heater_AO_Smith-IT-300_F_B" | element type "Indirect-Water-Heater_AO_Smith-IT-300_F_B" | 1 occurrence | material: materials ("RAL 9005", "Ral 9006 - Insulation", "Ral 9016")

Property sets
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 1310. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    System Classification = "Hydronic Supply" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Identity Data | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    OmniClass Number = "" (IFCTEXT)
    OmniClass Title = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Mark = "1" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Assembly Code = "D3010" (IFCTEXT)
    Assembly Description = "Energy Supply" (IFCTEXT)
    BIM Content Developer = "CAD & Company" (IFCTEXT)
    BIM Content Developer URL = "http://www.cadcompany.nl/" (IFCTEXT)
    CE-PIN = "" (IFCTEXT)
    Description = "Cuve Indirects Fournis d’un Échangeur" (IFCTEXT)
    Destination / Pays = "France" (IFCTEXT)
    Fabricant No. = "E 7110" (IFCTEXT)
    Guide de Produit = "https://www.aosmithinternational.com/sites/aosmithinternational.com/files/PDF-ALL/Instruction-manual-IT300-NL-UK-FR.pdf" (IFCTEXT)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCTEXT)
    Model = "IT 300 F B" (IFCTEXT)
    Nombre de modèle du produit (EAN) = "8717449181758" (IFCTEXT)
    OmniClass Number = "23.75.00.00" (IFCTEXT)
    OmniClass Title = "Climate Control (HVAC)" (IFCTEXT)
    Spécifications du Produit = "https://www.aosmithinternational.com/sites/aosmithinternational.com/files/FR%20pdf%20files/Specs-IT-FR.pdf" (IFCTEXT)
    URL = "http://www.aosmith.fr" (IFCTEXT)
  Phasing | properties | on 3 objects (2 IFCBUILDINGELEMENTPROXY, 1 IFCENERGYCONVERSIONDEVICE)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Manufacturer = "A.O. Smith Water Products Company b.v." (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Workspace = 860. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Diameter = 360. (IFCLENGTHMEASURE) [MILLI METRE]
    R = 25.4 (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.000115523821814436 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Volume = 4.34578346787956 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    hoogte workspace = 1870. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Diamètre (avec Isolation) = 360. (IFCLENGTHMEASURE) [MILLI METRE]
    Diamètre (sans Isolation) = 303. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur (avec Isolation) = 1370. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur (sans Isolation) = 1313. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de l'Alimentation en eau Froide = 75. (IFCLENGTHMEASURE) [MILLI METRE]
    Hauteur de la Sortie d'eau Chaude = 1310. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Profondeur = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    espace de travail = 860. (IFCLENGTHMEASURE) [MILLI METRE]
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "R1" (IFCIDENTIFIER)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Workspace" (IFCIDENTIFIER)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDING)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Model Properties | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Capacité - Cuve = 296. (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Capacité - Échangeur Inférieur = 8.9 (IFCVOLUMEMEASURE) [CUBIC_METRE]
    Charge Maximale au Sol = 413. (IFCREAL)
    Débit à 80ºC/60ºC - Échangeur Inférieur = 1978. (IFCREAL)
    Epaisseur d'Isolation = 57. (IFCLENGTHMEASURE) [MILLI METRE]
    Max. Température de l'eau - Réservoir = 368.15 (IFCREAL)
    Niveau du Son = "" (IFCTEXT)
    Perte de Pression à 80ºC/60ºC - Échangeur Inférieur = 1706.88 (IFCREAL)
    Pertes en Veille - tous les jours (24h) = 0. (IFCREAL)
    Pertes en Veille = 0. (IFCREAL)
    Poids à vide = 117. (IFCREAL)
    Pression de Service Maximale - Réservoir = 304800. (IFCREAL)
    Pression de Service Maximale - Échangeur Inférieur = 487680. (IFCREAL)
    Production Nominale - Échangeur Inférieur = 495139.879168647 (IFCREAL)
    Surface d'Échange de Chaleur - Échangeur Inférieur = 1.47 (IFCAREAMEASURE) [SQUARE_METRE]
    Température Maximale - Échangeur Inférieur = 383.15 (IFCREAL)
  Plumbing | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Raccord d'Alimentation en Eau Froide = 0.0833333333333333 (IFCREAL)
    Raccord de Sortie d'Eau Chaude = 0.0833333333333333 (IFCREAL)
    Raccord de la Soupape de Vidange = 0.0625 (IFCREAL)
  General | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    1er Entretien (check-up) = "3 mois après l'installation" (IFCTEXT)
    2ème Entretien (Entretien Général) = "12 mois après l'installation" (IFCTEXT)
    Garantie Pièces = "12 mois" (IFCTEXT)
    Garantie sur la Cuve = "36 mois" (IFCTEXT)
    Hauteur d'Emballage = 1510. (IFCLENGTHMEASURE) [MILLI METRE]
    Largeur d'Emballage = 780. (IFCLENGTHMEASURE) [MILLI METRE]
    Poids de Transport = 128. (IFCREAL)
    Profondeur d'Emballage = 780. (IFCLENGTHMEASURE) [MILLI METRE]
    Type d'Emballage = "Plastique et Bois" (IFCTEXT)
    l'Intervalle d'Entretien = "12 mois" (IFCTEXT)
  Mechanical - Flow | properties | on 1 object (1 IFCENERGYCONVERSIONDEVICE)
    Débit de vidage en Continu à ΔT = 28°C = 1413. (IFCREAL)
    Débit de vidage en Continu à ΔT = 44°C = 899. (IFCREAL)
    Débit de vidage en Continu à ΔT = 50°C = 791. (IFCREAL)
    Débit de vidage en Continu à ΔT = 55°C = 719. (IFCREAL)
    Débit de vidage en Continu à ΔT = 70°C = 565. (IFCREAL)
    Débit de vidage à ΔT = 28°C après 120 min. = 118.198189516822 (IFCREAL)
    Débit de vidage à ΔT = 28°C après 30 min. = 43.366410733988 (IFCREAL)
    Débit de vidage à ΔT = 28°C après 60 min. = 68.2985654393589 (IFCREAL)
    Débit de vidage à ΔT = 28°C après 90 min. = 93.2660348114513 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 120 min. = 75.2202401167707 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 30 min. = 27.5807547094826 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 60 min. = 43.4723547341524 (IFCREAL)
    Débit de vidage à ΔT = 44°C après 90 min. = 59.3286400921008 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 120 min. = 66.1796854360696 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 30 min. = 24.2964907043841 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 60 min. = 38.2457840593721 (IFCREAL)
    Débit de vidage à ΔT = 50°C après 90 min. = 52.2303920810816 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 120 min. = 60.1761920934166 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 30 min. = 22.0716667009304 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 60 min. = 34.7849467206663 (IFCREAL)
    Débit de vidage à ΔT = 55°C après 90 min. = 47.4629120736807 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 120 min. = 47.2863387400732 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 30 min. = 17.3395013602509 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 60 min. = 27.3335520424322 (IFCREAL)
    Débit de vidage à ΔT = 70°C après 90 min. = 37.2922880578919 (IFCREAL)
    Temps de réchauffement à ΔT = 28°C = "13" (IFCTEXT)
    Temps de réchauffement à ΔT = 44°C = "20" (IFCTEXT)
    Temps de réchauffement à ΔT = 50°C = "22" (IFCTEXT)
    Temps de réchauffement à ΔT = 55°C = "25" (IFCTEXT)
    Temps de réchauffement à ΔT = 70°C = 31 (IFCINTEGER)